# PAM Eye Measurements

Measurements

- Time Measurements
- Amplitude Measurements
- Clock Measurements
- Data Measurements
- SNDR Measurements
- PAM Measurements
- FFT Measurements
- User-Defined Measurements
- NRZ Eye Measurements
- PAM Eye Measurements
- Mask Test Commands
- Querying Measurement Results and Statistics

With option PAM analysis license, use the following commands to perform electrical and optical measurements on Pulse Amplitude Modulation (PAM) waveforms. Other commands are available for performing PAM Measurements.

- :MEASure:EYE:PAM:EHEight (Eye Heights)
- :MEASure:EYE:PAM:ELEVel (Eye Levels)
- :MEASure:EYE:PAM:ESKew (Eye Skews)
- :MEASure:EYE:PAM:EWIDth (Eye Widths)
- :MEASure:EYE:PAM:LEVel (PAM Levels)
- :MEASure:EYE:PAM:LINearity (Linearity)
- :MEASure:EYE:PAM:OVERshoot (Overshoot)
- :MEASure:EYE:PAM:PP (Levels Peak-Peak)
- :MEASure:EYE:PAM:PPAMplitude (Pk-Pk Amplitude)
- :MEASure:EYE:PAM:RMS (Levels RMS)
- :MEASure:EYE:PAM:SKEW (Levels Skews)
- :MEASure:EYE:PAM:UNDershoot (Undershoot)
- :MEASure:EYE:PAM:VECLosure (Vertical Eye Closure)