# :MEASure:PAM:LEVel:LEVel

PAM Levels Commands

- :MEASure:PAM:LEVel
- :MEASure:PAM:LEVel:FAVorite
- :MEASure:PAM:LEVel:LEVel
- :MEASure:PAM:LEVel:LOCation?
- :MEASure:PAM:LEVel:REGion
- :MEASure:PAM:LEVel:SOURce
- :MEASure:PAM:LEVel:STATus?
- :MEASure:PAM:LEVel:STATus:DETails?
- :MEASure:PAM:LEVel:STATus:REASon?
- :MEASure:PAM:LEVel:UREFerence:STATe
- :MEASure:PAM:LEVel:UREFerence:VALue

## Command Syntax

    :MEASure:PAM:LEVel:LEVel {LEVel0 | LEVel1 | LEVel2 | LEVel3}

## Query Syntax

    :MEASure:PAM:LEVel:LEVel?

## Description

Selects the level of a PAM or NRZ signal that will be measured when the `:MEASure:PAM:LEVel` parent command is sent. PAM4 signals have four possible levels: 0, 1, 2, and 3. PAM3 signals have three possible levels: 0, 1, and 2. NRZ signals have two possible levels: 0 and 1.

Arguments | Description
--- | ---
LEVel3 | Selects level 3. |
LEVel2 | Selects level 2.
LEVel1 | Selects level 1.
LEVel0 | Selects level 0.

## Example Command Sequence

    :MEASure:PAM:LEVel:LEVel LEVel2