# :MEASure:HORizontal:SLEWrate:EDIRection

Slew Rate Commands

- :MEASure:HORizontal:SLEWrate
- :MEASure:HORizontal:SLEWrate:EDIRection
- :MEASure:HORizontal:SLEWrate:FAVorite
- :MEASure:HORizontal:SLEWrate:LOCation?
- :MEASure:HORizontal:SLEWrate:OCCurrences
- :MEASure:HORizontal:SLEWrate:REGion
- :MEASure:HORizontal:SLEWrate:SOURce
- :MEASure:HORizontal:SLEWrate:STATus?
- :MEASure:HORizontal:SLEWrate:STATus:DETails?
- :MEASure:HORizontal:SLEWrate:STATus:REASon?
- :MEASure:HORizontal:SLEWrate:UREFerence:STATe
- :MEASure:HORizontal:SLEWrate:UREFerence:VALue

## Command Syntax

    :MEASure:HORizontal:SLEWrate:EDIRection {RISing | FALLing}

## Query Syntax

    :MEASure:HORizontal:SLEWrate:EDIRection?

## Description

For the slew rate measurement, specifies the waveform's edges to be measured: rising or falling edges.

## Example Command Sequence

This sequence sets up the measurement on rising edges only.

    :MEASure:HORizontal:SLEWrate:SOURce CHAN1_1
    :MEASure:HORizontal:SLEWrate:EDIRection RISing
      //  Perform measurement
    :MEASure:HORizontal:SLEWrate
    :MEASure:HORizontal:SLEWrate?