# :SOURce:NOISe:RN

Simulated and AWG Commands

- :SOURce:AMPLitude
- :SOURce:CDIVide
- :SOURce:DIFFerential
- :SOURce:FILTer:CUToff
- :SOURce:FILTer:RTIMe
- :SOURce:FILTer:STATe
- :SOURce:FILTer:TYPE
- :SOURce:FNAMe
- :SOURce:FORMat
- :SOURce:FOTWo:JITTer
- :SOURce:FOTWo:STATe
- :SOURce:FUNCtion
- :SOURce:INVert
- :SOURce:JITTer:BLIMit
- :SOURce:JITTer:BLSTate
- :SOURce:JITTer:DRJ?
- :SOURce:JITTer:DRN?
- :SOURce:JITTer:RJ
- :SOURce:JITTer:STATe
- :SOURce:LEVel
- :SOURce:NOISe:RN
- :SOURce:NOISe:STATe
- :SOURce:OENable
- :SOURce:OFFSet
- :SOURce:PATTern
- :SOURce:PLENgth
- :SOURce:PWIDth
- :SOURce:SEED
- :SOURce:SKEW
- :SOURce:SRATe
- :SOURce:SSC:FREQuency
- :SOURce:SSC:PATTern
- :SOURce:SSC:PERCent
- :SOURce:SSC:PHASe
- :SOURce:SSC:PPM
- :SOURce:SSC:STATe
- :SOURce:SSC:STYPe
- :SOURce:WTYPe

## Command Syntax

    :SOURceN:NOISe:RN  <RN>

<RN> is a double.

Where N identifies a simulated instrument's specific channel in the form "<connection1-8>_<ch1-8>" (for example, `SOURce4_2`). With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>" (for example, `SOURce3` which is the same as `SOURce1_3`).

## Query Syntax

    :SOURceN:NOISe:RN?

## Description

On simulated instruments, specifies the amount of Random Noise (RN) to be added to the indicated source waveform. Enter the value in volts (electrical waveforms) or Watts (optical waveforms). To apply the RN to the waveform, use the `:SOURce:NOISe:STATe` command.