# :FUNCtion:PARameters:DFEQualizer:PROPtimize:TAPS

DFE Parameters Commands

- :FUNCtion:PARameters:DFEQualizer:ATARgets
- :FUNCtion:PARameters:DFEQualizer:BANDwidth
- :FUNCtion:PARameters:DFEQualizer:BANDwidth:AUTO
- :FUNCtion:PARameters:DFEQualizer:BWMode
- :FUNCtion:PARameters:DFEQualizer:CLKDelay
- :FUNCtion:PARameters:DFEQualizer:DTHReshold
- :FUNCtion:PARameters:DFEQualizer:LTARget
- :FUNCtion:PARameters:DFEQualizer:PRESets
- :FUNCtion:PARameters:DFEQualizer:PRESets:SELections?
- :FUNCtion:PARameters:DFEQualizer:PROPtimize
- :FUNCtion:PARameters:DFEQualizer:PROPtimize:BMAX
- :FUNCtion:PARameters:DFEQualizer:PROPtimize:BMIN
- :FUNCtion:PARameters:DFEQualizer:PROPtimize:DELay
- :FUNCtion:PARameters:DFEQualizer:PROPtimize:LENGth
- :FUNCtion:PARameters:DFEQualizer:PROPtimize:LTMagnitudes
- :FUNCtion:PARameters:DFEQualizer:PROPtimize:MCURsor
- :FUNCtion:PARameters:DFEQualizer:PROPtimize:SAMPlitude
- :FUNCtion:PARameters:DFEQualizer:PROPtimize:SAVE
- :FUNCtion:PARameters:DFEQualizer:PROPtimize:SAVE:FILE
- :FUNCtion:PARameters:DFEQualizer:PROPtimize:TAPS
- :FUNCtion:PARameters:DFEQualizer:SEED
- :FUNCtion:PARameters:DFEQualizer:SEED:RTIMe
- :FUNCtion:PARameters:DFEQualizer:SEED:VALue
- :FUNCtion:PARameters:DFEQualizer:SOUTput
- :FUNCtion:PARameters:DFEQualizer:TAPS
- :FUNCtion:PARameters:DFEQualizer:TAPS:AUTO
- :FUNCtion:PARameters:DFEQualizer:TAPS:COUNt
- :FUNCtion:PARameters:DFEQualizer:TAPS:LLIMit
- :FUNCtion:PARameters:DFEQualizer:TAPS:RECalculate
- :FUNCtion:PARameters:DFEQualizer:TAPS:ULIMit
- :FUNCtion:PARameters:DFEQualizer:TLUNits
- :FUNCtion:PARameters:DFEQualizer:UTARget
- :FUNCtion:PARameters:DFEQualizer:VTAPs
- :FUNCtion:PARameters:DFEQualizer:WIDTh

## Command Syntax

    :FUNCtionN:PARameters:DFEQualizer:PROPtimize:TAPS  "tap_value, tap_value, …"

The command argument is a string of comma separated list of real numbers (individual tap value).

Where N identifies one of up to 64 possible operators {1:64} that can be defined as part of a math function. The operators are numbered in the order that they were originally added to the function.

## Query Syntax

    :FUNCtionN:PARameters:DFEQualizer:PROPtimize:TAPS?

## Query Response

    1.4582E-02,9.1E-05,1.85E-04

## Description

When `:FUNCtion:PARameters:DFEQualizer:PROPtimize` is `ON` and `:FUNCtion:PARameters:DFEQualizer:TAPS:AUTO` is `OFF`, use this command to manually enter tap values for an optimized pulse response. For example, for three taps you might enter:

    :FUNCtion1:PARameters:DFEQualizer:PROPtimize:TAPS "1.4582E-02,9.1E-05,1.85E-04"

Pulse response optimization (`:FUNCtion:PARameters:DFEQualizer:PROPtimize`) must be on to use this command.