# Operation Status Registers

Operation Status Registers Commands

- :STATus:ADERegister:EVENt?
- :STATus:ADERegister:ENABle
- :STATus:CALibration:EVENt?
- :STATus:CALibration:ENABle
- :STATus:CLIPped:ALL:CONNection:BANK:EVENt?
- :STATus:CLIPped:ALL:CONNection:BANK:ENABle
- :STATus:CLIPped:ALL:CONNection:EVENt?
- :STATus:CLIPped:ALL:CONNection:ENABle
- :STATus:CLIPped:ALL:EVENt?
- :STATus:CLIPped:ALL:ENABle
- :STATus:CLIPped:EVENt?
- :STATus:CLIPped:ENABle
- :STATus:LTESt:EVENt?
- :STATus:LTESt:ENABle
- :STATus:OPERation:EVENt?
- :STATus:OPERation:ENABle
- :STATus:OVERload:ALL:CONNection:BANK:EVENt?
- :STATus:OVERload:ALL:CONNection:BANK:ENABle
- :STATus:OVERload:ALL:CONNection:EVENt?
- :STATus:OVERload:ALL:CONNection:ENABle
- :STATus:OVERload:ALL:EVENt?
- :STATus:OVERload:ALL:ENABle
- :STATus:OVERload:EVENt?
- :STATus:OVERload:ENABle
- :STATus:TRIGger:EVENt?
- :STATus:TRIGger:ENABle

The Operation Status Register is a mid-level summary register in the status reporting structure. It contains summary bits that monitor activity in the other status registers and queues. The Operation Status Register is a live register. That is, its summary bits are set and cleared by the presence and absence of a summary bit from other event registers or queues.

Like other status registers, there is an event register (see `:STATus:OPERation:EVENt?`) that shows events and an enable register (see `:STATus:OPERation:ENABle`) that allows these events to pass on to bit 7 (OPER) of the Status Byte Registers.

Operation Status Register Bits
Bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
Bit Weight | 32,768 | 16,384 | 8,192 | 4,096 | 2,048 | 1,024 | 512 | 256 | 128 | 64 | 32 | 16 | 8 | 4 | 2 | 1
Event Register | — | CAL | OVLD-ALL | OVLD | — | — | LTEST | CLIP-ALL | CLIP | — | — | — | — | — | TRIG | ADER
Enable Register |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Sets | to Bit 7 (OPER) of Status Byte Register

The Operation Status Register, depending on the respective enable register masks, can collect information from these reporting registers:

- :STATus:CALibration:EVENt?
- :STATus:OVERload:ALL:EVENt?
- :STATus:OVERload:EVENt?
- :STATus:LTESt:EVENt?
- :STATus:CLIPped:ALL:EVENt?
- :STATus:CLIPped:EVENt?
- :STATus:TRIGger:EVENt?
- :STATus:ADERegister:EVENt?