# Message 10

## Message

"10. setting is at limit"

## Description

This is a general message that indicates that the specified control or setting was set to its limit. For example, this message would read "Timebase Scale is at limit" if you adjusted the seconds-per-division too low. Or, the message would read "Leading Digits is at limit" if you set the minimum number of Consecutive Identical Digits (CID) too high for Jitter amplitude analysis measurements.