# :FUNCtion:PARameters:DDEMbed:BSPan?

DeEmbed (4 port) Parameters Commands

- :FUNCtion:PARameters:DDEMbed:ALIGn
- :FUNCtion:PARameters:DDEMbed:BANDwidth
- :FUNCtion:PARameters:DDEMbed:BLIMit
- :FUNCtion:PARameters:DDEMbed:BSPan?
- :FUNCtion:PARameters:DDEMbed:CFRequency
- :FUNCtion:PARameters:DDEMbed:DRESult
- :FUNCtion:PARameters:DDEMbed:FNAMe
- :FUNCtion:PARameters:DDEMbed:IMPulse
- :FUNCtion:PARameters:DDEMbed:MEASsim
- :FUNCtion:PARameters:DDEMbed:RCORr
- :FUNCtion:PARameters:DDEMbed:RESolution
- :FUNCtion:PARameters:DDEMbed:SPAN
- :FUNCtion:PARameters:DDEMbed:STEP

## Query Syntax

    :FUNCtionN:PARameters:DDEMbed:BSPan?

Where N identifies one of up to 64 possible operators {1:64} that can be defined as part of a math function. The operators are numbered in the order that they were originally added to the function.

## Query Response

<frequency_span> is a double.

## Description

When the `BANDpass` filter type is selected (see `:FUNCtion:PARameters:DDEMbed:BLIMit`), this query returns the span of the bandpass filter.