# :MEASure:CLOCk:PPWidth:PTYPe

Pulse Width - Pulse Width Commands

- :MEASure:CLOCk:PPWidth
- :MEASure:CLOCk:PPWidth:FAVorite
- :MEASure:CLOCk:PPWidth:LOCation?
- :MEASure:CLOCk:PPWidth:PTYPe
- :MEASure:CLOCk:PPWidth:OCCurrences
- :MEASure:CLOCk:PPWidth:REGion
- :MEASure:CLOCk:PPWidth:SOURce
- :MEASure:CLOCk:PPWidth:STATus?
- :MEASure:CLOCk:PPWidth:STATus:DETails?
- :MEASure:CLOCk:PPWidth:STATus:REASon?
- :MEASure:CLOCk:PPWidth:UREFerence:STATe
- :MEASure:CLOCk:PPWidth:UREFerence:VALue

## Command Syntax

    :MEASure:CLOCk:PPWidth:PTYPe {POSitive | NEGative}

## Query Syntax

    :MEASure:CLOCk:PPWidth:PTYPe?

## Description

For the Pulse Width - Pulse Width measurement, specifies whether positive or negative pulse widths are measured.

POSitive
  Positive pulse width is defined as the time from the middle threshold of the first rising edge to the middle threshold of the next falling edge.
NEGative
  Negative pulse width is defined as the time from the middle threshold of the first falling edge to the middle threshold of the next rising edge.

## Example Command Sequence

This sequence sets up the measurement on rising edges only.

    :MEASure:CLOCk:PPWidth:SOURce CHAN1_1
    :MEASure:CLOCk:PPWidth:PTYPe POSitive
      //  Perform measurement
    :MEASure:CLOCk:PPWidth
    :MEASure:CLOCk:PPWidth?