# :DIFF:EYE:UIXRange

:DIFF EYE Commands

- :DIFF EYE Commands
- :DIFF:EYE:BITS
- :DIFF:EYE:CCOunt
- :DIFF:EYE:CURSor
- :DIFF:EYE:CWINdow
- :DIFF:EYE:DISPlay
- :DIFF:EYE:PATTern
- :DIFF:EYE:UIXPosition
- :DIFF:EYE:UIXRange
- :DIFF:EYE:UUNits
- :DIFF:EYE:XPOSition
- :DIFF:EYE:XSCale

## Command Syntax

    :DIFFN:EYE:UIXRange <time_in_UI>

Where N identifies a specific differential waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 differential waveform 3 (from the pairing of channels 3 and 4) is `DIFF5_3`.

<time_in_UI> is a double in UI (unit interval) units.

## Query Syntax

    :DIFFN:EYE:UIXRange?

## Description

Sets the differential waveform N horizontal time range (width) of the real-time eye display in UI units.

This command directly affects the real-time eye's horizontal time/div setting in seconds (see the `:DIFF:EYE:XSCale` command).

To set the horizontal position (center display location) of the real-time eye display in UI units, use the `:DIFF:EYE:UIXPosition` command.

Only the center UI is valid for the recovered clock edge. You can display up to 10 UIs to show context before and after the center UI.