# :CALibrate:CHANnel:ENABled

:CALibrate Channel Commands

- :CALibrate:CHANnel:ENABled
- :CALibrate:CHANnel:NOISe?
- :CALibrate:CHANnel:STATus?
- :CALibrate:CHANnel:STATus:DETails?
- :CALibrate:CHANnel:STATus:DTEMperature?
- :CALibrate:CHANnel:STATus:TIME?

## Command Syntax

    :CALibrate:CHANnelN:ENABled {ENABled | DISabled}

Where N identifies a specific channel in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, connection 4 channel 2 is `CHANnel4_2`.

## Query Syntax

    :CALibrate:CHANnelN:ENABled?

## Description

Enables or disables a vertical calibration for the indicated instrument's input channel.

ENABled
  Selects all calibrations be performed.
DISabled
  Prevents all calibrations from being performed.

Use the child queries listed in the following table to return details about the current calibration.

Status String Child Queries
Status String | Child Query to Send
--- | ---
Time of last calibration, Time change since last calibration, and Temperature change since last calibration | `:CALibrate:CHANnel:STATus:DETails?`
Change in temperature | `:CALibrate:CHANnel:STATus:DTEMperature?`
Change in Time | `:CALibrate:CHANnel:STATus:TIME?`

## Query Response

    {ENAB | DIS}

ENAB
  Indicates that all calibrations are selected.
DIS
  Indicates that all calibrations are disabled.