# :CMODe:UNAMe

:CMODe General Commands

- :CMODe:COLor
- :CMODe:CWINdow
- :CMODe:DISPlay
- :CMODe:PATTern:FILE:GCODe
- :CMODe:PATTern:FILE:NAME
- :CMODe:PATTern:FILE:RELoad
- :CMODe:PATTern:INVert
- :CMODe:PATTern:KPATtern
- :CMODe:PATTern:MODE
- :CMODe:SIGNal:TYPE
- :CMODe:SNOise:CALibrate
- :CMODe:SNOise:SNValue:LEVel{0:3}?
- :CMODe:STATus?
- :CMODe:UNAMe

## Command Syntax

    :CMODeN:UNAMe <string>

Where N identifies a specific common-mode waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 common-mode waveform 3 (from the pairing of channels 3 and 4) is `CMODe5_3`.

## Query Syntax

    :CMODeN:UNAMe?

## Description

Assigns a custom user name to a common-mode waveform. User names are helpful because they identify what a waveform represents rather than the oscilloscope's input channel. For example, you could assign user name "DUT 3, CM Output" to common-mode waveform 2C. User names can be 25 characters or less and are displayed on the screen and on screen captures. To remove a custom user name, re-create it using an empty string.

Custom user names can by created for other waveforms using the following commands:

- `:CHANnel:UNAMe`
- `:DIFF:UNAMe`
- `:CGMemory:UNAMe`
- `:FUNCtion:UNAMe`
- `:WMEMory:UNAMe`

## Example Command Sequence

    :CMODe3:UNAMe "DUT 3, CM Output"