# :MEASure:VERTical:CPOWer:AIMPedance

Carrier Power Commands

- :MEASure:VERTical:CPOWer
- :MEASure:VERTical:CPOWer:AIMPedance
- :MEASure:VERTical:CPOWer:FAVorite
- :MEASure:VERTical:CPOWer:LOCation?
- :MEASure:VERTical:CPOWer:REGion
- :MEASure:VERTical:CPOWer:RIMPedance
- :MEASure:VERTical:CPOWer:SOURce
- :MEASure:VERTical:CPOWer:STATus?
- :MEASure:VERTical:CPOWer:STATus:DETails?
- :MEASure:VERTical:CPOWer:STATus:REASon?
- :MEASure:VERTical:CPOWer:UREFerence:STATe
- :MEASure:VERTical:CPOWer:UREFerence:VALue

## Command Syntax

    :MEASure:VERTical:CPOWer:AIMPedance {ON | OFF | 1 | 0}

## Query Syntax

    :MEASure:VERTical:CPOWer:AIMPedance?

## Query Response

    {1 | 0}

## Description

For the Carrier Power measurement (see `:MEASure:VERTical:CPOWer`), this command turns on or off the Auto Reference Impedance. When off, you can specify the reference impedance with the `:MEASure:VERTical:CPOWer:RIMPedance` command.