# :LTESt:ACQuire:CTYPe:WAVeforms

:LTESt Acquisition Commands

- :LTESt:ACQuire:CTYPe
- :LTESt:ACQuire:CTYPe:SAMPles
- :LTESt:ACQuire:CTYPe:WAVeforms
- :LTESt:ACQuire:SIMage:FNAMe
- :LTESt:ACQuire:SIMage:FNAMe:AUPDate
- :LTESt:ACQuire:SIMage:FNAMe:USTandard
- :LTESt:ACQuire:SIMage:FTYPe?
- :LTESt:ACQuire:SIMage:IMETadata
- :LTESt:ACQuire:SIMage:INVert
- :LTESt:ACQuire:SIMage:MONochrome
- :LTESt:ACQuire:SIMage:SINClude
- :LTESt:ACQuire:SIMage:STATe
- :LTESt:ACQuire:SIMage:WINDow
- :LTESt:ACQuire:STATe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:CHANnel:FTYPe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:STATe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:CMODe{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:CMODe:FTYPe
- :LTESt:ACQuire:SWAVeform:CMODe{N}:STATe
- :LTESt:ACQuire:SWAVeform:CMODe{N}:WMEMory WMEMory{1:8}
- :LTESt:ACQuire:SWAVeform:DIFF{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:DIFF:FTYPe
- :LTESt:ACQuire:SWAVeform:DIFF{N}:STATe
- :LTESt:ACQuire:SWAVeform:DIFF{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:STATe
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:RESet

## Command Syntax

    :LTESt:ACQuire:CTYPe:WAVeforms <number>

<number> is an int.

## Query Syntax

    :LTESt:ACQuire:CTYPe:WAVeforms?

## Description

Enters the number of waveforms required to stop an acquisition limit test that is based on waveforms. Use the `:LTESt:ACQuire:CTYPe` command to select to test based on waveforms.

## Example Command Sequence

This example sequence of commands erases display memory and sets up an acquisition limit test.

    :ACQuire:CDISplay
    :LTESt:ACQuire:CTYPe WAVeforms
    :LTESt:ACQuire:CTYPe:WAVeforms 200
    :LTESt:ACQuire:STATe ON
    :ACQuire:RUN
    *OPC?
    …  //  Your code to synchronize execution timing.

## Parent Command

- `:LTESt:ACQuire:CTYPe`