# :NETWorks:TRACe:NETWork

:NETWorks:TRACe General Commands

- :NETWorks:TRACe:COLor
- :NETWorks:TRACe:CWINdow
- :NETWorks:TRACe:DISPlay
- :NETWorks:TRACe:NETWork
- :NETWorks:TRACe:OPERator
- :NETWorks:TRACe:PARameter
- :NETWorks:TRACe:STATus?
- :NETWorks:TRACe:UNAMe?

## Command Syntax

    :NETWorks:TRACeN:NETWork SPMemory{1:4}

Where N identifies a specific trace and must be selected from 1 to 128 {1:128}.

## Query Syntax

    :NETWorks:TRACe{1:128}:NETWork?

## Description

This command specifies an S-parameter or transfer function memory from which to select a response to assign to a trace. One of four S-parameter/transfer function file memories can be selected as the source for a response. To select the actual S-parameter/transfer function response to assign to the trace, use the `:NETWorks:TRACe:PARameter` command.