# :MEASure:HORizontal:HTIMe:STATus:REASon?

Hold Time Commands

- :MEASure:HORizontal:HTIMe
- :MEASure:HORizontal:HTIMe:CEDirection
- :MEASure:HORizontal:HTIMe:DEDirection
- :MEASure:HORizontal:HTIMe:FAVorite
- :MEASure:HORizontal:HTIMe:LOCation?
- :MEASure:HORizontal:HTIMe:OCCurrences
- :MEASure:HORizontal:HTIMe:REGion
- :MEASure:HORizontal:HTIMe:SOURce
- :MEASure:HORizontal:HTIMe:STATus?
- :MEASure:HORizontal:HTIMe:STATus:DETails?
- :MEASure:HORizontal:HTIMe:STATus:REASon?
- :MEASure:HORizontal:HTIMe:UREFerence:STATe
- :MEASure:HORizontal:HTIMe:UREFerence:VALue

## Query Syntax

    :MEASure:HORizontal:HTIMe:STATus:REASon?

## Query Response

Refer to the table Common Reasons for INV or QUES Status.

## Description

Returns a string that explains the reason for a failed `:MEASure:HORizontal:HTIMe` measurement. If the measurement was successful, a null string is returned.

Additional information about the failure may be available using the `:MEASure:HORizontal:HTIMe:STATus:DETails?` sibling query. Use the `:MEASure:HORizontal:HTIMe:STATus?` parent query to determine if the measurement has failed.

## See Also

- Measurement Errors