# :STATus:CLIPped:ALL:CONNection:BANK:EVENt?

Operation Status Registers Commands

- :STATus:ADERegister:EVENt?
- :STATus:ADERegister:ENABle
- :STATus:CALibration:EVENt?
- :STATus:CALibration:ENABle
- :STATus:CLIPped:ALL:CONNection:BANK:EVENt?
- :STATus:CLIPped:ALL:CONNection:BANK:ENABle
- :STATus:CLIPped:ALL:CONNection:EVENt?
- :STATus:CLIPped:ALL:CONNection:ENABle
- :STATus:CLIPped:ALL:EVENt?
- :STATus:CLIPped:ALL:ENABle
- :STATus:CLIPped:EVENt?
- :STATus:CLIPped:ENABle
- :STATus:LTESt:EVENt?
- :STATus:LTESt:ENABle
- :STATus:OPERation:EVENt?
- :STATus:OPERation:ENABle
- :STATus:OVERload:ALL:CONNection:BANK:EVENt?
- :STATus:OVERload:ALL:CONNection:BANK:ENABle
- :STATus:OVERload:ALL:CONNection:EVENt?
- :STATus:OVERload:ALL:CONNection:ENABle
- :STATus:OVERload:ALL:EVENt?
- :STATus:OVERload:ALL:ENABle
- :STATus:OVERload:EVENt?
- :STATus:OVERload:ENABle
- :STATus:TRIGger:EVENt?
- :STATus:TRIGger:ENABle

## Query Syntax

    :STATus:CLIPped:ALL:CONNectionN:BANKM:EVENt?

Where N identifies one of up to eight {1:8} connections that can be used for instruments.

Where M identifies a bank of up to 8 channels. Current oscilloscopes supported by Infiniium are all less than 8 channels, so M is always "1" (or not used).

## Description

Reads the Clipped All Connection Bank register to see which channels that have reported ADC clipping since the last time the register was read.

Reading the register once will clear the status for all channels.

Reporting of event register bits in the status register system is controlled by the mask loaded into the enable register. All true event bits, that are enabled, are logically "OR"ed, which results in setting true bit M-1 (BANKM) of the Clipped All Connection Register.

Clipped All Connection Bank Register Commands
Register | Read | Write | Command
--- | --- | --- | ---
Event | ♦ |  | :STATus:CLIPped:ALL:CONNection:BANK:EVENt?
Enable (mask) | ♦ | ♦ | :STATus:CLIPped:ALL:CONNection:BANK:ENABle

Clipped All Connection Bank Register Bits
Bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
Bit Weight | 32768 | 16384 | 8192 | 4096 | 2048 | 1024 | 512 | 256 | 128 | 64 | 32 | 16 | 8 | 4 | 2 | 1
Event Register | — | — | — | — | — | — | — | — | CH8 | CH7 | CH6 | CH5 | CH4 | CH3 | CH2 | CH1
Enable Register |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Sets | to Bit M-1 (CLIPM) of Clipped All Connection Register

## Bit Definitions

CH1-CH8
  A true indicates the channel has reported ADC clipping since the last time the register was read. If the oscilloscope has fewer than eight channels, only those bits are used.