# :WMEMory:INTerpolate:STATus:REASon?

:WMEMory General Commands

- :WMEMory:CLEar
- :WMEMory:COLor
- :WMEMory:CWINdow
- :WMEMory:DISPlay
- :WMEMory:DSTatus?
- :WMEMory:DSTatus:REASon?
- :WMEMory:INTerpolate:FACTor
- :WMEMory:INTerpolate:METHod
- :WMEMory:INTerpolate:STATus?
- :WMEMory:INTerpolate:STATus:REASon?
- :WMEMory:PATTern:FILE:GCODe
- :WMEMory:PATTern:FILE:NAME
- :WMEMory:PATTern:FILE:RELoad
- :WMEMory:PATTern:INVert
- :WMEMory:PATTern:KPATtern
- :WMEMory:PATTern:MODE
- :WMEMory:SIGNal:TYPE
- :WMEMory:STATus?
- :WMEMory:TTIMebase
- :WMEMory:UNAMe
- :WMEMory:UNAMe:UFName

## Query Syntax

    :WMEMoryN:INTerpolate:STATus:REASon?

Where N identifies one of eight {1:8} possible waveform memories. For example, `:WMEMory4`.

## Query Response

    <string>

## Description

If the status of the specified waveform memory's interpolation on load is invalid (see `:WMEMory:INTerpolate:STATus?`), this query returns a description of the invalid status.

If the status of the specified waveform memory interpolation on load is correct, this query returns an empty string.