# :CGMemory:LOAD

:CGMemory Loading Commands

- :CGMemory:FILE:LOAD
- :CGMemory:FILE:NAME
- :CGMemory:LOAD
- :CGMemory:LOAD:SOURce

## Command Syntax

    :CGMemoryN:LOAD

Where N identifies one of eight {1:8} color grade memories. For example, the color grade memory 2 would be identified as `:CGMemory2`.

## Description

Loads the selected waveform source into the indicated eye-memory location. Use the `:CGMemory:LOAD:SOURce` command to select the source. Use the `:CGMemory:DISPlay` command to display the eye-memory waveform.

To load a color grade-gray scale file into color grade memory, use the `:CGMemory:FILE:LOAD` and `:CGMemory:FILE:NAME` commands.

## Example Command Sequence

    :CGMemory2:LOAD:SOURce CHAN1_1
    :CGMemory2:LOAD
    :CGMemory2:DISPlay ON

## Child Commands

- `:CGMemory:LOAD:SOURce` specifies the source waveform on which to perform the measurement.