# :TRIGger:QUALify:ZONE:ISZLogic

:TRIGger Qualify Commands

- :TRIGger:QUALify:FOQualify
- :TRIGger:QUALify:MEASure:LLIMit
- :TRIGger:QUALify:MEASure:LOCation
- :TRIGger:QUALify:MEASure:REGion
- :TRIGger:QUALify:MEASure:ULIMit
- :TRIGger:QUALify:MODE
- :TRIGger:QUALify:STATe
- :TRIGger:QUALify:ZONE:ISZLogic
- :TRIGger:QUALify:ZONE:ZONE{N}:LOGic
- :TRIGger:QUALify:ZONE:ZONE{N}:SOURce
- :TRIGger:QUALify:ZONE:ZONE{N}:STATe
- :TRIGger:QUALify:ZONE:ZONE{N}:X
- :TRIGger:QUALify:ZONE:ZONE{N}:Y

## Command Syntax

    :TRIGger:QUALify:ZONE:ISZLogic  {AND | OR}

## Query Syntax

    :TRIGger:QUALify:ZONE:ISZLogic?

## Description

When zone qualified triggers are enabled (see `:TRIGger:QUALify:MODE`), this command specifies the Inter Signal Zone Logic, that is, the logic used when combining the zones of different signals.