# :STATus:CLIPped:ALL:CONNection:ENABle

Operation Status Registers Commands

- :STATus:ADERegister:EVENt?
- :STATus:ADERegister:ENABle
- :STATus:CALibration:EVENt?
- :STATus:CALibration:ENABle
- :STATus:CLIPped:ALL:CONNection:BANK:EVENt?
- :STATus:CLIPped:ALL:CONNection:BANK:ENABle
- :STATus:CLIPped:ALL:CONNection:EVENt?
- :STATus:CLIPped:ALL:CONNection:ENABle
- :STATus:CLIPped:ALL:EVENt?
- :STATus:CLIPped:ALL:ENABle
- :STATus:CLIPped:EVENt?
- :STATus:CLIPped:ENABle
- :STATus:LTESt:EVENt?
- :STATus:LTESt:ENABle
- :STATus:OPERation:EVENt?
- :STATus:OPERation:ENABle
- :STATus:OVERload:ALL:CONNection:BANK:EVENt?
- :STATus:OVERload:ALL:CONNection:BANK:ENABle
- :STATus:OVERload:ALL:CONNection:EVENt?
- :STATus:OVERload:ALL:CONNection:ENABle
- :STATus:OVERload:ALL:EVENt?
- :STATus:OVERload:ALL:ENABle
- :STATus:OVERload:EVENt?
- :STATus:OVERload:ENABle
- :STATus:TRIGger:EVENt?
- :STATus:TRIGger:ENABle

## Command Syntax

    :STATus:CLIPped:ALL:CONNectionN:ENABle <mask>

<mask> is an integer, 0 to 65535, representing a mask for the bits in the event register.

## Query Syntax

    :STATus:CLIPped:ALL:CONNectionN:ENABle?

## Description

Enters a decimal-weighted value in the enable register that masks the ability to report bits in the Clipped All Connection Register (see `:STATus:CLIPped:ALL:CONNection:EVENt?`).

Clipped All Connection Register Commands
Register | Read | Write | Command
--- | --- | --- | ---
Event | ♦ |  | :STATus:CLIPped:ALL:CONNection:EVENt?
Enable (mask) | ♦ | ♦ | :STATus:CLIPped:ALL:CONNection:ENABle

Clipped All Connection Register Bits
Bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
Bit Weight | 32768 | 16384 | 8192 | 4096 | 2048 | 1024 | 512 | 256 | 128 | 64 | 32 | 16 | 8 | 4 | 2 | 1
Event Register | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | BANK1
Enable Register |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
Sets | to Bit N-1 (CONNN) of Clipped All Register

## Bit Definitions

BANK1
  A true indicates the channels on bank 1 reported ADC clipping since the last time the register was read.