# :WMEMory:INTerpolate:FACTor

:WMEMory General Commands

- :WMEMory:CLEar
- :WMEMory:COLor
- :WMEMory:CWINdow
- :WMEMory:DISPlay
- :WMEMory:DSTatus?
- :WMEMory:DSTatus:REASon?
- :WMEMory:INTerpolate:FACTor
- :WMEMory:INTerpolate:METHod
- :WMEMory:INTerpolate:STATus?
- :WMEMory:INTerpolate:STATus:REASon?
- :WMEMory:PATTern:FILE:GCODe
- :WMEMory:PATTern:FILE:NAME
- :WMEMory:PATTern:FILE:RELoad
- :WMEMory:PATTern:INVert
- :WMEMory:PATTern:KPATtern
- :WMEMory:PATTern:MODE
- :WMEMory:SIGNal:TYPE
- :WMEMory:STATus?
- :WMEMory:TTIMebase
- :WMEMory:UNAMe
- :WMEMory:UNAMe:UFName

## Command Syntax

    :WMEMoryN:INTerpolate:FACTor <factor>

<factor> is an integer.

Where N identifies one of eight {1:8} possible waveform memories. For example, `:WMEMory4`.

## Query Syntax

    :WMEMoryN:INTerpolate:FACTor?

## Description

For the selected waveform memory, this command specifies a factor (integer value) that determines the number of interpolated points Infiniium between sampled points in the input waveform. To select the interpolation on load method, use the `:WMEMory:INTerpolate:METHod` command.