# :DIFF:EYE:WINDow:TRACking

:DIFF EYE Commands

- :DIFF EYE Commands
- :DIFF:EYE:BITS
- :DIFF:EYE:CCOunt
- :DIFF:EYE:CURSor
- :DIFF:EYE:CWINdow
- :DIFF:EYE:DISPlay
- :DIFF:EYE:PATTern
- :DIFF:EYE:UIXPosition
- :DIFF:EYE:UIXRange
- :DIFF:EYE:UUNits
- :DIFF:EYE:XPOSition
- :DIFF:EYE:XSCale

## Command Syntax

    :DIFFN:EYE:WINDow:TRACking  {{ON | 1} | {OFF | 0}}

Where N identifies a specific differential waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 differential waveform 3 (from the pairing of channels 3 and 4) is `DIFF5_3`.

## Query Syntax

    :DIFFN:EYE:WINDow:TRACking?

## Query Response

    {1 | 0}

## Description

Specifies whether a signal tracks the global eye window definition or uses its own eye window definition.

The global eye window definition is set using the `:MEASure:EYE:WINDow` commands (see Eye Window Configuration Commands).

## Example Command Sequence

    :DIFF1:EYE:WINDow:TRACking OFF
    :DIFF1:EYE:WINDow:METHod EOPening
    :DIFF1:EYE:WINDow:LEFT 40.0
    :DIFF1:EYE:WINDow:RIGHt 60.0