# :MEASure:PAM:EYE:ESTiming

PAM Analysis Setup Commands

- :MEASure:PAM:AMPLitude:UNITs
- :MEASure:PAM:EYE:ELMethod
- :MEASure:PAM:EYE:ESTiming
- :MEASure:PAM:EYE:PPERcent
- :MEASure:PAM:EYE:TIME:LTDefinition
- :MEASure:PAM:EYE:TIME:UNITs

## Command Syntax

    :MEASure:PAM:EYE:ESTiming {CEYE | PELevel}

## Query Syntax

    :MEASure:PAM:EYE:ESTiming?

## Description

Configures the timing for sampling the signal data for all PAM measurements. Use this setting to match the timing method used by a receiver. For signals with skewed eyes, measurements results will vary depending on this setting. This setting does not apply to PAM measurements.

Arguments | Description
--- | ---
CEYE | Sampling timing is based on the location of the center eye (labeled Eye 1/2 in the following picture). This is the default setting.
PELevel | Sampling timing is independently based on the location of each of the three eyes.