# :MEASure:JITTer:NOISe:VECLosure:STATus:DETails?

Noise VEC Commands

- :MEASure:JITTer:NOISe:VECLosure?
- :MEASure:JITTer:NOISe:VECLosure:EYE
- :MEASure:JITTer:NOISe:VECLosure:STATus?
- :MEASure:JITTer:NOISe:VECLosure:STATus:DETails?
- :MEASure:JITTer:NOISe:VECLosure:STATus:REASon?

## Query Syntax

    :MEASure:JITTerN:NOISe:VECLosure:STATus:DETails?

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Description

Returns a string that may provide additional details for a failed `:MEASure:JITTer:NOISe:VECLosure?` measurement. If the measurement was successful, a null string is returned.

For a basic description of a measurement failure, use the `:MEASure:JITTer:NOISe:VECLosure:STATus:REASon?` sibling query. Use the `:MEASure:JITTer:NOISe:VECLosure:STATus?` parent query to determine if the measurement has failed.

## See Also

- Measurement Errors