# :CMODe:EYE:XPOSition

:CMODe EYE Commands

- :CMODe EYE Commands
- :CMODe:EYE:BITS
- :CMODe:EYE:CCOunt
- :CMODe:EYE:CURSor
- :CMODe:EYE:CWINdow
- :CMODe:EYE:DISPlay
- :CMODe:EYE:PATTern
- :CMODe:EYE:UIXPosition
- :CMODe:EYE:UIXRange
- :CMODe:EYE:UUNits
- :CMODe:EYE:WINDow:COPY
- :CMODe:EYE:WINDow:LEFT
- :CMODe:EYE:WINDow:METHod
- :CMODe:EYE:WINDow:RIGHt
- :CMODe:EYE:WINDow:TRACking
- :CMODe:EYE:WINDow:WIDTh
- :CMODe:EYE:XPOSition
- :CMODe:EYE:XSCale

## Command Syntax

    :CMODeN:EYE:XPOSition <time>

Where N identifies a specific common-mode waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 common-mode waveform 3 (from the pairing of channels 3 and 4) is `CMODe5_3`.

<time> is a double.

## Query Syntax

    :CMODeN:EYE:XPOSition?

## Description

Sets the common-mode waveform N horizontal time position (center display location) of the real-time eye display.

This command directly affects the real-time eye's horizontal position setting in UI (unit interval) units (see the `:CMODe:EYE:UIXPosition` command).

To set the horizontal time scale of the real-time eye display in seconds-per-division, use the `:CMODe:EYE:XSCale` command.