# :MEASure:EYE:PAM:PPAMplitude:UNITs

:PAM Pk-Pk Amplitude Commands

- :MEASure:EYE:PAM:PPAMplitude
- :MEASure:EYE:PAM:PPAMplitude:FAVorite
- :MEASure:EYE:PAM:PPAMplitude:LOCation?
- :MEASure:EYE:PAM:PPAMplitude:SOURce
- :MEASure:EYE:PAM:PPAMplitude:STATus?
- :MEASure:EYE:PAM:PPAMplitude:STATus:DETails?
- :MEASure:EYE:PAM:PPAMplitude:STATus:REASon?
- :MEASure:EYE:PAM:PPAMplitude:THRatio
- :MEASure:EYE:PAM:PPAMplitude:UNITs

## Command Syntax

    :MEASure:EYE:PAM:PPAMplitude:UNITs {WATT | DBM | VOLT}

## Query Syntax

    :MEASure:EYE:PAM:PPAMplitude:UNITs?

## Description

Sets the amplitude units for the Pk-Pk Amplitude measurement (`:MEASure:EYE:PAM:PPAMplitude`). Units can be Watts (`WATT`) or dBM (`DBM`) for an optical signal and Volts (`VOLT`) for an electrical signal.