# :CGMemory:SIGNal:TYPE

:CGMemory General Commands

- :CGMemory:CLEar
- :CGMemory:COLor
- :CGMemory:CWINdow
- :CGMemory:DISPlay
- :CGMemory:DSTatus?
- :CGMemory:DSTatus:REASon?
- :CGMemory:PERSistence
- :CGMemory:SIGNal:TYPE
- :CGMemory:STATus?
- :CGMemory:UNAMe
- :CGMemory:UNAMe:UFName

## Command Syntax

    :CGMemoryN:SIGNal:TYPE {UNSPecified | NRZ | PAM3 | PAM4}

## Query Syntax

    :CGMemoryN:SIGNal:TYPE?

## Description

Specifies the signal type that is stored in color-grade gray-scale memory. The default value is unspecified (`UNSPecified`).

The PAM options are available when the PAM-N analysis software license is installed.