# :MEASure:HORizontal:HTIMe:DEDirection

Hold Time Commands

- :MEASure:HORizontal:HTIMe
- :MEASure:HORizontal:HTIMe:CEDirection
- :MEASure:HORizontal:HTIMe:DEDirection
- :MEASure:HORizontal:HTIMe:FAVorite
- :MEASure:HORizontal:HTIMe:LOCation?
- :MEASure:HORizontal:HTIMe:OCCurrences
- :MEASure:HORizontal:HTIMe:REGion
- :MEASure:HORizontal:HTIMe:SOURce
- :MEASure:HORizontal:HTIMe:STATus?
- :MEASure:HORizontal:HTIMe:STATus:DETails?
- :MEASure:HORizontal:HTIMe:STATus:REASon?
- :MEASure:HORizontal:HTIMe:UREFerence:STATe
- :MEASure:HORizontal:HTIMe:UREFerence:VALue

## Command Syntax

    :MEASure:HORizontal:HTIMe:DEDirection {RISing | FALLing | BOTH}

## Query Syntax

    :MEASure:HORizontal:HTIMe:DEDirection?

## Description

For the :MEASure:HORizontal:HTIMe measurement, specifies which data signal edges to include in the measurement.

The `BOTH` option means both rising and falling data signal edges are included in the measurement.

## Example Command Sequence

This sequence sets up the measurement using both data signal edges and the falling clock signal edge.

    :MEASure:HORizontal:HTIMe:SOURce1 CHAN1_1
    :MEASure:HORizontal:HTIMe:SOURce2 CHAN1_2
    :MEASure:HORizontal:HTIMe:DEDirection BOTH
    :MEASure:HORizontal:HTIMe:CEDirection FALLing
    //  Perform measurement
    :MEASure:HORizontal:HTIMe
    :MEASure:HORizontal:HTIMe?