# :NETWorks:TRACe:YUNits?

:NETWorks:TRACe Scaling Commands

- :NETWorks:TRACe:XLEFt?
- :NETWorks:TRACe:XPOSition?
- :NETWorks:TRACe:XREFerence?
- :NETWorks:TRACe:XRIGht?
- :NETWorks:TRACe:XSCale?
- :NETWorks:TRACe:XUNits?
- :NETWorks:TRACe:YBOTtom?
- :NETWorks:TRACe:YOFFset?
- :NETWorks:TRACe:YRANge?
- :NETWorks:TRACe:YSCale?
- :NETWorks:TRACe:YTOP?
- :NETWorks:TRACe:YUNits?

## Query Syntax

    :NETWorks:TRACeN:YUNits?

Where N identifies a specific trace and must be selected from 1 to 128 {1:128}.

## Query Response

    {OHM | VOLT | PERC | DEGR | SEC | DEC}

## Description

Queries the Y-axis units-of-measurement for the indicated S-parameter trace. The returned strings are described in the following table.

Returned Values with Displayed Content Window Graph
Returned String | Y-Axis Units | Content Window Graphs
--- | --- | ---
S-Parameters
DEC | Decibels | Freq-Mag
DEGR | Degrees | Phase
SEC | Seconds | GrpDelay