# :CMODe:EYE:WINDow:WIDTh

:CMODe EYE Commands

- :CMODe EYE Commands
- :CMODe:EYE:BITS
- :CMODe:EYE:CCOunt
- :CMODe:EYE:CURSor
- :CMODe:EYE:CWINdow
- :CMODe:EYE:DISPlay
- :CMODe:EYE:PATTern
- :CMODe:EYE:UIXPosition
- :CMODe:EYE:UIXRange
- :CMODe:EYE:UUNits
- :CMODe:EYE:WINDow:COPY
- :CMODe:EYE:WINDow:LEFT
- :CMODe:EYE:WINDow:METHod
- :CMODe:EYE:WINDow:RIGHt
- :CMODe:EYE:WINDow:TRACking
- :CMODe:EYE:WINDow:WIDTh
- :CMODe:EYE:XPOSition
- :CMODe:EYE:XSCale

## Command Syntax

    :CMODeN:EYE:WINDow:WIDTh<percent>

Where N identifies a specific common-mode waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 common-mode waveform 3 (from the pairing of channels 3 and 4) is `CMODe5_3`.

<percent> is a double.

## Query Syntax

    :CMODeN:EYE:WINDow:WIDTh?

## Description

When the "At Clock Time" eye window determination method is selected (see `:CMODe:EYE:WINDow:METHod`), this command specifies the UI percentage width about the recovered clock location to use as the eye window. A zero percent for this setting means only the recovered clock location is used.

This command is equivalent to the settings in the Eye tab of the Configure Measurements dialog box.