# :TRIGger:CHANnel:LEVel:FIFTy

:TRIGger General Commands

- :TRIGger:AUX:LEVel
- :TRIGger:AUX:LEVel:FIFTy
- :TRIGger:CHANnel:HTHReshold
- :TRIGger:CHANnel:LEVel
- :TRIGger:CHANnel:LEVel:FIFTy
- :TRIGger:CHANnel:LTHReshold
- :TRIGger:FORCe
- :TRIGger:HYSTeresis
- :TRIGger:MODE
- :TRIGger:SWEep

## Command Syntax

    :TRIGger:CHANnelN:LEVel:FIFTy

Where N identifies a specific channel in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, connection 4 channel 2 is `CHANnel4_2`.

## Description

Automatically sets the channel's trigger level to 50% of the input signal amplitude.

This is the same a pushing the oscilloscope's front panel Trigger Level knob.