# :MEASure:EYE:PAM:RMS:STATus:REASon?

Level RMS Commands

- :MEASure:EYE:PAM:RMS
- :MEASure:EYE:PAM:RMS:FAVorite
- :MEASure:EYE:PAM:RMS:LEVel
- :MEASure:EYE:PAM:RMS:LOCation?
- :MEASure:EYE:PAM:RMS:SOURce
- :MEASure:EYE:PAM:RMS:STATus?
- :MEASure:EYE:PAM:RMS:STATus:DETails?
- :MEASure:EYE:PAM:RMS:STATus:REASon?

## Query Syntax

    :MEASure:EYE:PAM:RMS:STATus:REASon?

## Query Response

Refer to the table "Common Reasons for INV or QUES Status".

## Description

Returns a string that explains the reason for a failed `:MEASure:EYE:PAM:RMS` measurement. If the measurement was successful, a null string is returned.

Additional information about the failure may be available using the `:MEASure:EYE:PAM:RMS:STATus:DETails?` sibling query. Use the `:MEASure:EYE:PAM:RMS:STATus?` parent query to determine if the measurement has failed.

## See Also

- Measurement Errors