# :MEASure:PAM:RFTime:TRANsition

PAM Rise/Fall Times Commands

- :MEASure:PAM:RFTime
- :MEASure:PAM:RFTime:EDIRection
- :MEASure:PAM:RFTime:FAVorite
- :MEASure:PAM:RFTime:LOCation?
- :MEASure:PAM:RFTime:OCCurrences
- :MEASure:PAM:RFTime:REGion
- :MEASure:PAM:RFTime:SOURce
- :MEASure:PAM:RFTime:STATus?
- :MEASure:PAM:RFTime:STATus:DETails?
- :MEASure:PAM:RFTime:STATus:REASon?
- :MEASure:PAM:RFTime:TRANsition
- :MEASure:PAM:RFTime:UREFerence:STATe
- :MEASure:PAM:RFTime:UREFerence:VALue

## Command Syntax

    :MEASure:PAM:RFTime:TRANsition {TRANsition01 | TRANsition02 | TRANsition03
       | TRANsition12 | TRANsition13 | TRANsition23}

## Query Syntax

    :MEASure:PAM:RFTime:TRANsition?

## Description

Selects the level-to-level transition of a PAM signal that will be measured when the `:MEASure:PAM:RFTime` parent command is sent. PAM4 signals have six possible level-to-level transitions: 0-1, 0-2, 0-3, 1-2, 1-3, and 2-3. PAM3 signals have three possible level-to-level transitions: 0-1, 0-2, and 1-2.

Whether the edge is rising or falling is specified by the `:MEASure:PAM:RFTime:EDIRection` command.