# :MEASure:DATA:DTIerror:UREFerence:STATe

Data TIE Commands

- :MEASure:DATA:DTIerror
- :MEASure:DATA:DTIerror:EYE
- :MEASure:DATA:DTIerror:FAVorite
- :MEASure:DATA:DTIerror:LOCation?
- :MEASure:DATA:DTIerror:OCCurrences
- :MEASure:DATA:DTIerror:REGion
- :MEASure:DATA:DTIerror:SOURce
- :MEASure:DATA:DTIerror:STATus?
- :MEASure:DATA:DTIerror:STATus:DETails?
- :MEASure:DATA:DTIerror:STATus:REASon?
- :MEASure:DATA:DTIerror:TIEFilter
- :MEASure:DATA:DTIerror:TIEFilter:DFACtor
- :MEASure:DATA:DTIerror:TIEFilter:SHAPe
- :MEASure:DATA:DTIerror:TIEFilter:STARt
- :MEASure:DATA:DTIerror:TIEFilter:STOP
- :MEASure:DATA:DTIerror:TIEFilter:TYPE
- :MEASure:DATA:DTIerror:UNITs
- :MEASure:DATA:DTIerror:UREFerence:STATe
- :MEASure:DATA:DTIerror:UREFerence:VALue

## Command Syntax

    :MEASure:DATA:DTIerror:UREFerence:STATe {ON | OFF | 1 | 0}

## Query Syntax

    :MEASure:DATA:DTIerror:UREFerence:STATe?

## Query Response

    {1 | 0}

## Description

Enables or disables a user-defined horizontal reference location near which a one-measurement-per-acquisition measurement is made.

When a user-defined horizontal reference location is enabled, the `:MEASure:DATA:DTIerror:UREFerence:VALue` command specifies its time location with respect to the trigger (t = 0) location.