# :CMODe:EYE:CWINdow

:CMODe EYE Commands

- :CMODe EYE Commands
- :CMODe:EYE:BITS
- :CMODe:EYE:CCOunt
- :CMODe:EYE:CURSor
- :CMODe:EYE:CWINdow
- :CMODe:EYE:DISPlay
- :CMODe:EYE:PATTern
- :CMODe:EYE:UIXPosition
- :CMODe:EYE:UIXRange
- :CMODe:EYE:UUNits
- :CMODe:EYE:WINDow:COPY
- :CMODe:EYE:WINDow:LEFT
- :CMODe:EYE:WINDow:METHod
- :CMODe:EYE:WINDow:RIGHt
- :CMODe:EYE:WINDow:TRACking
- :CMODe:EYE:WINDow:WIDTh
- :CMODe:EYE:XPOSition
- :CMODe:EYE:XSCale

## Command Syntax

    :CMODeN:EYE:CWINdow TIME{1:4}

Where N identifies a specific common-mode waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 common-mode waveform 3 (from the pairing of channels 3 and 4) is `CMODe5_3`.

## Query Syntax

    :CMODeN:EYE:CWINdow?

## Description

The `:CMODe:EYE:CWINdow` command allows you to assign a common-mode real-time eye waveform to a Waveform content window.

In Infiniium, several different types of content windows exist. Common-mode channel waveforms can only be displayed in a Waveform (`TIME`) content window of which there is currently only one available.

Command Arguments and Content Windows
Argument | Displayed Waveform Content Window | Number of Available Windows | Scale Units
--- | --- | --- | ---
Programmatically | Via Front Panel
TIME{1:4} | Waveform | 4 | 4 | Y-Axis: Volts or Watts (linear scale) X-Axis: seconds