# Time Measurements

Subtopics

- Burst Interval
- Burst Period
- Burst Width
- Delta Time
- Duty Cycle
- Fall Time
- Frequency
- Hold Time
- N-Period
- Period
- Phase
- Pulse Count
- Pulse Width
- Rise Time
- Setup Time
- Slew Rate
- Time at Max
- Time at Min
- Time at Amplitude
- Time at Edge

With the exception of the jitter measurements, Oscilloscope time measurements are designed for single-valued waveforms. When a jitter measurement is selected, the instrument's measurement database is enabled. Jitter is the only oscilloscope measurement that uses the database as a source. The waveform data that is sampled is accumulated in the measurement database. In order to view this data, you must select the color grade (or gray scale) display persistence mode.

## Toolbar 1 of 4

Rise Time
Fall Time
Period
Setup Time
Hold Time
N-Period

## Toolbar 2 of 4

Frequency
Pulse Width
Pulse Count
Δ Time
Duty Cycle
Phase

## Toolbar 3 of 4

Slew Rate
Time at Amplitude
Time at Edge
Time at Max
Time at Min
Burst Width

## Toolbar 4 of 4

Burst Interval
Burst Period

## PAM-Compatible Measurements on NRZ Time Toolbar

Some, but not all, of the NRZ measurements listed in the Time and Amplitude tabs of the measurements toolbar can be used on PAM waveforms. The measurements that you can use are shown in the following tables.

### Compatible

- Time at Max
- Time at Min
- Time at Amplitude

### Compatible
(Depending on Waveform)

- Rise Time
- Fall Time
- Δ Time
- Time at Edge

### Incompatible

- Period
- Frequency
- Pulse Width
- Duty Cycle
- Phase