# PAM Analysis Setup Commands

PAM Measurements

- PAM Analysis Setup Commands
- :MEASure:PAM:LEVel
- :MEASure:PAM:RFTime
- :MEASure:PAM:RMS

- :MEASure:PAM:AMPLitude:UNITs (Amplitude Units)
- :MEASure:PAM:EYE:ELMethod (Eye Center Location)
- :MEASure:PAM:EYE:ESTiming (Receiver Sample Timing)
- :MEASure:PAM:EYE:PPERcent (Eye Level Width)
- :MEASure:PAM:EYE:TIME:LTDefinition (Time of Level)
- :MEASure:PAM:EYE:TIME:UNITs (Time Units)

Effect on Various Measurements
Measurement Commands | :MEASure Child Commands
--- | ---
Receiver Sample Timing (ESTiming) | Eye Center Timing (ELMethod) | Eye Level Width (PPERcent) | Time of Level (LTDefinition) | Time Units (TIME UNITs) | Amplitude Units (AMPLitude UNITs)
Symbol definitions: ♦ = setting affects measurement. ◊ = setting may affect measurement.
Eye Heights | ♦ | ♦ | ♦ |  |  | ♦
Eye Levels | ◊ | ◊ | ♦ | ♦ |  | ♦
Levels Peak-Peak | ◊ | ◊ | ♦ | ♦ |  | ♦
Levels RMS | ◊ | ◊ | ♦ | ♦ |  | ♦
Level Skews | ♦ | ♦ | ♦ | ♦ | ♦ |
Eye Levels | ♦ | ♦ | ♦ |  |  | ♦
Eye Skews | ♦ | ♦ | ♦ |  | ♦ |
Eye Widths | ♦ | ♦ |  |  | ♦ |
Linearity | ♦ | ♦ | ♦ | ♦ |  |