# :CHANnel:FILTer:ACQuisition:MODE

:CHANnel FILTer Commands

- :CHANnel FILTer Commands
- :CHANnel:FILTer:ACQuisition:BANDwidth
- :CHANnel:FILTer:ACQuisition:MODE
- :CHANnel:FILTer:BANDwidth
- :CHANnel:FILTer:CFRequency
- :CHANnel:FILTer:SPAN?
- :CHANnel:FILTer:TYPE

## Command Syntax

    :CHANnelN:FILTer:ACQuisition:MODE {MAX | CUSTom}

Where N identifies a specific channel in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, connection 4 channel 2 is `CHANnel4_2`.

## Query Syntax

    :CHANnelN:FILTer:ACQuisition:MODE?

## Description

For the oscilloscope input channel hardware bandwidth limit filter, this command selects either:

MAX
  The maximum available bandwidth.
CUSTom
  A custom limited bandwidth. Use the `:CHANnel:FILTer:ACQuisition:BANDwidth` command to specify the custom bandwidth.