# :DIFF:EYE:CWINdow

:DIFF EYE Commands

- :DIFF EYE Commands
- :DIFF:EYE:BITS
- :DIFF:EYE:CCOunt
- :DIFF:EYE:CURSor
- :DIFF:EYE:CWINdow
- :DIFF:EYE:DISPlay
- :DIFF:EYE:PATTern
- :DIFF:EYE:UIXPosition
- :DIFF:EYE:UIXRange
- :DIFF:EYE:UUNits
- :DIFF:EYE:XPOSition
- :DIFF:EYE:XSCale

## Command Syntax

    :DIFFN:EYE:CWINdow TIME{1:4}

Where N identifies a specific differential waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 differential waveform 3 (from the pairing of channels 3 and 4) is `DIFF5_3`.

## Query Syntax

    :DIFFN:EYE:CWINdow?

## Description

The `:DIFF{N}:EYE:CWINdow` command lets you assign a differential real-time eye waveform to a Waveform content window.

In Infiniium 2026, several different types of content windows exist. differential channel waveforms can only be displayed in a Waveform (`TIME`) content window of which there is currently only one available.

Command Arguments and Content Windows
Argument | Displayed Waveform Content Window | Number of Available Windows | Scale Units
--- | --- | --- | ---
Programmatically | Via Front Panel
TIME{1:4} | Waveform | 4 | 4 | Y-Axis: Volts or Watts (linear scale) X-Axis: seconds