# :MEASure:JITTer:JITTer:EDGE

Jitter Setup Commands

- :MEASure:JITTer:BSCale
- :MEASure:JITTer:GSCale
- :MEASure:JITTer:JITTer:ANALysis
- :MEASure:JITTer:JITTer:DIMensions
- :MEASure:JITTer:JITTer:DMAXimized
- :MEASure:JITTer:JITTer:EDGE
- :MEASure:JITTer:JITTer:EOPening
- :MEASure:JITTer:JITTer:EOPening:PROBability
- :MEASure:JITTer:JITTer:FLAG
- :MEASure:JITTer:JITTer:FLEad
- :MEASure:JITTer:JITTer:MODE
- :MEASure:JITTer:JITTer:NUINtervals
- :MEASure:JITTer:JITTer:PTYPe
- :MEASure:JITTer:JITTer:RJBandwidth
- :MEASure:JITTer:JITTer:RJComp
- :MEASure:JITTer:JITTer:RJCResult?
- :MEASure:JITTer:JITTer:RJCValue
- :MEASure:JITTer:JITTer:RJSTabilize
- :MEASure:JITTer:JITTer:RJSValue
- :MEASure:JITTer:JITTer:SMEThod
- :MEASure:JITTer:JITTer:TJBer
- :MEASure:JITTer:JITTer:UNITs
- :MEASure:JITTer:SOURce

## Command Syntax

    :MEASure:JITTerN:JITTer:EDGE {RISing | FALLing | BOTH}

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Query Syntax

    :MEASure:JITTerN:JITTer:EDGE?

## Description

This command selects whether jitter measurements are made on the `RISing` edge, the `FALLing` edge, or `BOTH` edges (rising and falling).

Jitter measurements performed on clock-type signals typically use a single edge setting, unless both edges of the clock are used to latch data.

In double data rate applications, this control should be set to `BOTH` edges.