# :FUNCtion:PARameters:GAUSsian:BANDwidth

Gaussian Parameters Commands

- :FUNCtion:PARameters:GAUSsian:BANDwidth
- :FUNCtion:PARameters:GAUSsian:IMPulse
- :FUNCtion:PARameters:GAUSsian:RTIMe
- :FUNCtion:PARameters:GAUSsian:STEP
- :FUNCtion:PARameters:GAUSsian:TFUNction

## Command Syntax

    :FUNCtionN:PARameters:GAUSsian:BANDwidth <cutoff_frequency>

<cutoff_frequency> is a double.

Where N identifies one of up to 64 possible operators {1:64} that can be defined as part of a math function. The operators are numbered in the order that they were originally added to the function.

## Query Syntax

    :FUNCtionN:PARameters:GAUSsian:BANDwidth?

## Description

Specifies the cutoff frequency in Hertz of a Gaussian filter operator (`:FUNCtion:FOPerator`).

## Example Command Sequence

    :FUNCtion2:FOPerator GAUSsian
    :FUNCtion2:PARameters:GAUSsian:BANDwidth 7.5E6
    :FUNCtion2:PARameters:GAUSsian:RTIMe 52.4E-12
    :FUNCtion2:COLor TCOLor4
    :FUNCtion2:DISPlay ON
    *OPC?
    …
                      //  Your code to synchronize execution timing.