# :NETWorks:TRACe:STATus?

:NETWorks:TRACe General Commands

- :NETWorks:TRACe:COLor
- :NETWorks:TRACe:CWINdow
- :NETWorks:TRACe:DISPlay
- :NETWorks:TRACe:NETWork
- :NETWorks:TRACe:OPERator
- :NETWorks:TRACe:PARameter
- :NETWorks:TRACe:STATus?
- :NETWorks:TRACe:UNAMe?

## Query Syntax

    :NETWorks:TRACeN:STATus?

Where N identifies a specific trace and must be selected from 1 to 128 {1:128}.

## Query Response

    {AVA | UNAV}

## Description

Queries the availability of a trace for use. A trace becomes available (`AVA`) after it is defined and displayed. Available traces are not shown in the Signals Palette. An available trace's waveform may or may not be displayed. A trace is unavailable (`UNAV`) unless it has been defined using all of the following three commands:

- `:NETWorks:TRACe:NETWork` command.
- `:NETWorks:TRACe:OPERator` command.
- `:NETWorks:TRACe:PARameter` command.

A trace does not have to be displayed to be available.