# :MEASure:JITTer:NOISe:PIR:STATus?

Noise PI (rms) Commands

- :MEASure:JITTer:NOISe:PIR?
- :MEASure:JITTer:NOISe:PIR:LEVel
- :MEASure:JITTer:NOISe:PIR:STATus?
- :MEASure:JITTer:NOISe:PIR:STATus:DETails?
- :MEASure:JITTer:NOISe:PIR:STATus:REASon?

## Query Syntax

    :MEASure:JITTerN:NOISe:PIR:STATus?

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Query Response

    {CORR | INV | QUES}

CORR
  The measurement result is correct.
INV
  The measurement result is invalid.
QUES
  The measurement result is questionable.

## Description

Queries the status of the `:MEASure:JITTer:NOISe:PIR?` measurement. Use the `:MEASure:JITTer:NOISe:PIR:STATus:REASon?` child query to determine the reason for an invalid or questionable measurement. Additional information about the failure may be available using the `:MEASure:JITTer:NOISe:PIR:STATus:DETails?` child query.

## See Also

- Measurement Errors