# :TRIGger:SWEep

:TRIGger General Commands

- :TRIGger:AUX:LEVel
- :TRIGger:AUX:LEVel:FIFTy
- :TRIGger:CHANnel:HTHReshold
- :TRIGger:CHANnel:LEVel
- :TRIGger:CHANnel:LEVel:FIFTy
- :TRIGger:CHANnel:LTHReshold
- :TRIGger:FORCe
- :TRIGger:HYSTeresis
- :TRIGger:MODE
- :TRIGger:SWEep

## Command Syntax

    :TRIGger:SWEep {AUTO | TRIGgered}

## Query Syntax

    :TRIGger:SWEep?

## Description

This command selects the trigger mode:

- `AUTO` — If the specified trigger conditions are not found, triggers are forced and acquisitions are made so that signal activity is displayed on the oscilloscope.
- `TRIGgered` — Triggers and acquisitions occur only when the specified trigger conditions are found.