# :NETWorks:DFILe:FILE:NAME

:NETWorks:DFILe Commands

- :NETWorks:DFILe Commands
- :NETWorks:DFILe:CLEar
- :NETWorks:DFILe:DSTatus?
- :NETWorks:DFILe:DSTatus:REASon?
- :NETWorks:DFILe:ENABle?
- :NETWorks:DFILe:FILE:LOAD
- :NETWorks:DFILe:FILE:NAME
- :NETWorks:DFILe:PTYPe?

## Command Syntax

    :NETWorks:DFILeN:FILE:NAME "filename"

Where N identifies one of four {1:4} memories. For example, `:NETWorks:DFILe2`.

## Query Syntax

    :NETWorks:DFILe:FILE:NAME?

## Query Response

    "filename"

## Description

Specifies the file (name, path, and extension) for recalling S-parameters into S-parameter memory. The default source folder is `%USER_DATA_DIR%`\S-Parameter Data. Use the `:NETWorks:DFILe:FILE:LOAD` command to actually load the file into memory. Use the query to determine the default S-parameter filename which is suggested based on the number of DUT ports.

Import File Types
File Type | Description
--- | ---
.ts2 | Touchstone 2 file. Single-ended and differential data
.s1p | Touchstone 1 file. One-port single-ended device data (S11 or S22)
.s2p | Touchstone 1 file. Two-port single-ended device data (S11, S21, S22, S12)
.s4p | Touchstone 1 file. Four-port single-ended device data
.s8p | Touchstone 1 file. Eight-port single-ended device data
.s12p | Touchstone 1 file. Twelve-port single-ended device data
.s16p | Touchstone 1 file. Sixteen-port single-ended device data
.txt | Identical to the .s1p file type except for the .txt filename extension.