# :MEASure:JITTer:NOISe:COUNt:LEVel

Noise Bit Count Commands

- :MEASure:JITTer:NOISe:COUNt?
- :MEASure:JITTer:NOISe:COUNt:LEVel
- :MEASure:JITTer:NOISe:COUNt:STATus?
- :MEASure:JITTer:NOISe:COUNt:STATus:DETails?
- :MEASure:JITTer:NOISe:COUNt:STATus:REASon?

## Command Syntax

    :MEASure:JITTerN:NOISe:COUNt:LEVel {LEVel0 | LEVel1}

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Query Syntax

    :MEASure:JITTerN:NOISe:COUNt:LEVel?

## Description

This command specifies the level for which the measurement value is returned.