# :TRIGger:CHANnel:LTHReshold

:TRIGger General Commands

- :TRIGger:AUX:LEVel
- :TRIGger:AUX:LEVel:FIFTy
- :TRIGger:CHANnel:HTHReshold
- :TRIGger:CHANnel:LEVel
- :TRIGger:CHANnel:LEVel:FIFTy
- :TRIGger:CHANnel:LTHReshold
- :TRIGger:FORCe
- :TRIGger:HYSTeresis
- :TRIGger:MODE
- :TRIGger:SWEep

## Command Syntax

    :TRIGger:CHANnelN:LTHReshold <level>

Where N identifies a specific channel in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, connection 4 channel 2 is `CHANnel4_2`.

<level> is a double.

## Query Syntax

    :TRIGger:CHANnelN:LTHReshold?

## Description

In the trigger modes that use upper and lower threshold levels (see `:TRIGger:MODE`), this command specifies the lower threshold level for a particular analog channel input.