# :MEASure:JITTer:JITTer:TFILter:TYPE

Jitter/Noise Advanced Setup Commands

- :MEASure:JITTer:JITTer:TFILter:DFACtor
- :MEASure:JITTer:JITTer:TFILter:SHAPe
- :MEASure:JITTer:JITTer:TFILter:STARt
- :MEASure:JITTer:JITTer:TFILter:STOP
- :MEASure:JITTer:JITTer:TFILter:TYPE
- :MEASure:JITTer:TFILter:STATe

## Command Syntax

    :MEASure:JITTerN:JITTer:TFILter:TYPE {LPFilter | BPFilter | HPFilter}

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Query Syntax

    :MEASure:JITTerN:JITTer:TFILter:TYPE?

## Description

This command specifies the TIE filter edge type: Low-pass, Band-pass, or High-pass.