# :CALibrate:CALibrator:DCOFfset

:CALibrate Calibrator Commands

- :CALibrate:CALibrator:AOENable
- :CALibrate:CALibrator:DCOFfset
- :CALibrate:CALibrator:ESPeed
- :CALibrate:CALibrator:MODE
- :CALibrate:CALibrator:PWIDth
- :CALibrate:CALibrator:SPULse

## Command Syntax

    :CALibrate:CALibrator:DCOFfset  <voltage>

<voltage> is a double.

## Query Syntax

    :CALibrate:CALibrator:DCOFfset?

## Description

When the DC level calibrator mode is selected (see `:CALibrate:CALibrator:MODE`), this command sets the DC voltage output on the oscilloscope's front-panel calibration output (Cal Out). This output can be used to:

- Manually verify the DC accuracy of a instrument's electrical channel calibration.
- Calibrate a probe.